**Iowa Repeater Council, Inc**.

Annual Survey

Form Notes

**Sponsor:**

Abbreviation is limited to 10 characters.

**Location:**

Site name: If there is a commonly referred to name enter it here (i.e. Ames water tower)

Directory Listing Area: For consistency please limit selection to the following list.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Burlington | Council Bluffs | Dubuque | North Central | Sioux City | Southwest |
| Cedar Rapids | Davenport | East Central | Northeast | South Central | Waterloo |
| Central | Des Moines | Mason City | Northwest | Southeast | West Central |

Region: Circle one

**Features:**

Check all that apply

**Transmit/Receive:**

Tx Power (Watts): Power out at transmitter

ERP (Watts): **E**ffective **R**adiated **P**ower from ERP worksheet

HAAT(Feet): **H**eight **A**bove **A**verage **T**errain from HAAT worksheet or software.

Site AMSL (Feet): Site elevation **A**bove **M**ean **S**ea **L**evel.

*Antenna*:

Bearing: If Directional enter Degrees. If Omni enter 0

Antenna Height AGL: Height of center of radiation **A**bove **G**round **L**evel in feet.

*Emission/Tone/Codes:*

|  |  |  |  |
| --- | --- | --- | --- |
| Emission Designators | | Tone/Code types: | |
| 20K0F3E | 5 kHz deviation FM Voice | CTCSS | Tone Squelch |
| 16K0F3E | 4 kHz deviation FM Voice | CDCSS | Digital Tone Squelch |
| 11K2F3E | 2.5 kHz deviation FM Voice | CALLSIGN | Callsign encoded in data stream |
| 8K10F1E | P25 PI C4FM Voice | P25 | NAC – Network Access Code |
| 9K80D7W | P25 PII fixed end 2-slot TDMA | DMR | Color Code |
| 7K60FXE | DMR 2-slot TDMA Voice | NXDN | RAN - Repeater Access Number |
| 6K00F7W | ICOM D-Star | FUSION | DSQ – Digital Squelch Code |
| 150KF1D | DSTAR DD mode | VIDEO | NTSC, MPEC, etc. |
| 8K30F1E | NXDN 12.5 kHz voice |  |  |
| 4K00F1E | NXDN 6.25 kHz voice |  |  |
| 9K36F7W | Yaesu Fusion |  | **Return Form to:** |
| 6M00A5J | NTSC Video |  | Frequency Coordinator |
| 20K0D1E | TETRA PowerTrunk 4-slot TDMA voice |  | Iowa Repeater Council, Inc |
| 20K0D1W | TETRA PowerTrunk 4-slot TDMA mixed |  | Roland Newton KC0IEA |
| 11K2F2D | PACKET AFSK 1200bps 2.5 kHz Deviation |  | PO Box 2222 |
| 16K0F2D | PACKET AFSK 1200bps 4 kHz Deviation |  | Ames, Iowa 50010-2222 |
| 20K0F2D | PACKET AFSK 1200bps 5 kHz Deviation |  | coordinator@iowarepeater.org |